# Guard grate ASG.P, load-bearing up to 200 kg

**Guard grate** in accordance with DGUV regulation 103- 007, rectangular, made from 1.4307 (AISI 304 L)   
stainless steel, universally applicable and retrofittable under manhole covers.

**Guard grate** manufactured from angle profile, loadbearing up to 200 kg, with hinges and gas pressure   
spring for easy opening and closing.

**Support** made of angle profile, for internal bolted fixing under the manhole cover.

Guard grate for mounting under the manhole cover and above or next to the climbing system.

Both grate and support are shielded arc-welded and acid bath cleaned before washing, drying and surface passivation.

Fixing material included.

**Options:**

➤ 1.4404 (AISI 316 L) stainless steel

➤ Removable grate for round manholes

➤ Non-standard sizes