# Guard grate ASG for manhole covers, load bearing up to 150 kg

# **Guard grate** in accordance with DGUV regulation 103- 007, rectangular, made from 1.4307 (AISI 304 L) stainless steel, universally applicable and retrofittable under manhole covers.

**Grate** made of perforated plate with 5 mm perforations in staggered rows, load bearing capacity 150 kg,   
hinged and lockable, provided for locking with a customer provided padlock.

**Support,** made of angle profile, for internal bolted fixing under the manhole cover.

Guard grate for mounting under the manhole cover and above the climbing system.

Both grate and support are shielded arc-welded and acid bath cleaned before washing,   
drying and surface passivation.

Fixing material included.

**Options:**

➤ 1.4404 (AISI 316 L) stainless steel

➤ Lockable version

➤ Removable grate for round manholes

➤ Non-standard sizes