# Catch basin CT for manhole covers

**Catch basin,** rectangular in shape, made of 1.4307 (AISI 304 L) stainless steel, universally applicable, for retrofitting under manhole covers as protection against ingress of harmful chemicals, liquid or similar substances into the manhole.

Custom-made to suit the specific local conditions.

**The cover** is made of stainless steel plate, with a centrally raised profile, removable, with two handles.

**The frame** consists of an angle section designed as an outlet channel, provided for bolted fixing inside the manhole under the manhole cover, with integrated ¾“ hose nozzle, for on-site connection to an outlet pipe. Fixing material and drinking water approved silicone as sealing between the wall and frame included.

Cover and frame shielded arc-welded and acid bath cleaned before washing, drying and surface passivation.

**Options:**

➤ 1.4404 (AISI 316 L) stainless steel

➤ Air vent DN 150

➤ Lockable version