# Fold-back entrance aid EH K

**Fold-back entrance aid,** made of 1.4307 (AISI 304 L) stainless steel, for safety access ladders with   
300 mm, 400 mm, 500 mm width.

In accordance with DIN 3620.

**Note:** The 1.1 m projection required according to DIN 19572 is not achieved with this design variant   
of the entrance aid.

Manhole width = mm [with round manhole entrances only possible for 300 mm wide access ladders].

Completely shielded arc welded, acid-treated in a pickling bath and passivated.

**Options:**

➤ 1.4404 (AISI 316 L) stainless steel