# Window with thermo glass and reversible frame F3

**Casement window,** swivel window, ready for installation, made from two-sheet special 1.4301 (AISI 304) stainless steel profile with intermediate special plastic core to prevent thermal conduction, thermally insulated according to EN 10077, Uf = 2.70 W/(m²\*K), fittings specially E-Look galvanized, stainless steel handle set.

**Blind frame,** circumferential, made from special profile, designed for dowelling into window soffit, including fixing material.

**Sash frame,** made from Z-profile, integrated fittings. Multiple locking via handle set. Two rebate gaskets.

Glazing bead invisibly fastened. Machine ground **surface finish.**

**Dry glazing** with insulation glass, without KTW approval

## Door opening options:

➤ Hinges on left

➤ Hinges on right

## Options:

➤ 1.4404 (AISI 316 L) stainless steel

➤ Secure to prevent forced access according to  
DIN EN 1627, RC3, galvanized fittings, only possible with wet glazing

➤ Special glazing (e.g. security glass)

➤ Multi-wing window

➤ Outside window sill made from stainless steel

➤ Water chamber window (with drain holes towards the dry side, with wet glazing, KTW approved)

➤ Lockable handle set provided for profile cylinder

➤ Other designs available on request