# Prefabricated manhole FGS 1

# **Prefabricated manhole,** completely made of 1.4307 (AISI 304 L) stainless steel, watertight, with entrance and installation opening in accordance with DVGW Standard W 122. Robust casing, diameter: 1900/2500 mm, head room: 2000 mm, height of domes: 800 mm, total height: 3290/3400 mm, bottom made of tear pattern plate (slip resistance R 11 in accordance with DIN 51130) with inclination to the pump sump, for bolted fixing on a customer-provided concrete foundation, with the following stainless steel components:

➤ Manhole cover, round type, designed as an entrance opening, 800 mm diameter, with rubber seal, with air vent DN 150 (order no. 108/GDR)

➤ Manhole cover, round type, designed as an installation opening, 800 mm diameter, with rubber seal (order no. 108/GDR), or according to the well head size

➤ Safety access ladder, width 300 mm, vertical installation, length 2850/3130 mm

➤ Fold-back/extensible entrance aid

➤ Ventilating chimney DN 150, 200 mm, ending above manhole bottom

➤ FF-piece, DN as a pipe duct, length

200 mm, welded in the casing, floor distance: 800 mm

➤ Cable duct, diameter: mm, floor distance: 1000 mm

➤ Holders for control panel

➤ Pump sump, 300 mm diameter, welded to the bottom, covered by a perforated stainless steel plate, with handle

➤ Lifting eyes

➤ Fixing material

Completely shielded arc welded, acid-treated in a pickling bath and passivated, including all built-in components.

## Options:

➤ Well head, DN in accordance with technical data sheet BKF 1, welded to the manhole bottom

➤ Provided for optional ventilator

➤ 1.4404 (AISI 316 L) stainless steel

## Fields of application:

Prefabricated stainless steel manholes are watertight and frost-proof. They are applied in flood areas and areas with a high groundwater level. They are quickly installed, permanently corrosion resistant and maintenance-free.

## Note:

A concrete foundation is required for watertight prefabricated manholes installed below ground water level.