Fall arrestor S5c in accordance with DIN EN 353-1

**Fall arrestor** type S5c with self-unfolding safety belttype HSE-BFD and spring safety hooks certified and

approved by “TÜV SÜD PRODUCT SERVICE GmbH“, CE 0123 in accordance with DIN EN 353-1, suitable for

HUBER safety guard rail FSS.

**Options:**

➤ Safety belt in accordance with EN 361, form A (breastshoulder-crotch belt), suitable for safety guard rail.