# Round Access Cover TT8a with screwed joints

## Maintenance opening, especially for the field of potable water supply, pressure-tight up to a water gauge of 5 m.

## Access cover, pressure-tight up to a water gauge of 5 m, ready for installation, round, completely made from 1.4307 (AISI 304 L) stainless steel, with intermediate sealing suitable for the specific application, can be lined on both sides.

**Blank cover** with lock and two handles for easy operation, connected with the frame by means of screwed joints.

**Frame,** designed as F-piece with centrally welded wall flange, provided for embedding in concrete.   
Frame with lifting eyes.

Blank cover and frame shielded arc-welded and acid bath cleaned before washing, drying and surface passivation.

**Options:**

➤ 1.4404 (AISI 316 L) stainless steel

➤ Centrally installed inspection window, inside diameter: 150 mm, with or without window wiper

➤ Sanding of frame parts in contact with concrete

➤ Stable maintenance-free hinges screwed to the frame, can be lined on both sides.   
(Please indicate the door opening option.)

## Application:

➤ Drinking water (KTW certified sealing)

➤ Wastewater (rubber seal SBR)

➤ Biogas (rubber seal EPDM E628 70 ± 5 Shore)