# Round Inspection Cover TT8b

## Sight glass in the bottom of water tanks, pressure-tight up to a water gauge of 10 m.

**Inspection cover,** pressure-tight up to a water gauge of 10 m, round, completely made from   
1.4404 (AISI 316 L) stainless steel, can be lined on both sides.

**Sight glass** with 15 mm thick safety glass, convex towards the pressure side.   
Sealing with two rubber seals. Clear sight diameter: 400 mm.

**Access duct cover** with centrally welded wall flange, provided for embedding in concrete.   
Wall flange dimensions: 616 mm.

Access duct cover shielded arc-welded, acid-treated in a pickling bath and passivated.

## Options:

➤ 1.4307 (AISI 304 L) stainless steel

➤ Sanding of wall pipe parts in contact with concrete